| SONATA(YF) >2012 > G 2.4 GDI > Body Electrical System > MTS System>Description and Operation |

Description

Mobile Telemetics System (MTS)
Hyundai motor companies are now faced with the task of shifting their paradigm from vehicle-centered services to customer valuecentered services, with the ultimate goal of securing global leadership in the fi eld of vehicle IT and telematics.
Hyundai Motor plans to achieve this by realizing a terminal platform fl exible to changes in IT technology, cooperating with global IT companies, creating an eco-system and providing the latest contents & services based on an open environment.
Blue Link is a dynamic, telematics technology that allows Hyundai vehicles to send—and receive—important and useful information.
The system uses an enhanced cellular network, with automatic roaming, that optimizes connections and prioritizes emergency requests.
With Blue Link you get…

- | Automatic emergency assistance, in the unfortunate event of a collision.

- | The convenience of point-of-interest search and navigation assistance, as well as the ability to remotely operate various vehicle features.

- | The peace of mind of self-diagnostic vehicle reports, and more.

Main Features

1. | TMU Concept : Registered driver request the Service from Call Center (Safety and Security, TBT service, etc.)

2. | GPS & CDMA Communication : Connect the Call Center by CDMA. Use Simple Navigation System by GPS & CDMA (Only Audio type).

3. | Integrate a Voice Recognition & Communication : User can operate the service by Speech Recognition (only Audio) User can use downloaded POI Data by CDMA (only AVN).

4. | Control BCM by Call Center Service : Door Lock/Unlock, Horn/Light, Remote Start/Stop be operate by Service.

Block Diagram

System Components

Using procedures

1. | Enrolling in Blue Link After the enrollment process, you can use to access your Blue Link preferences.

For more detail procedure, please refer to the Blue Link owner's manual.

2. | Subscribe the Blue Link Packages Blue Link services come in three groupings, or packages:

Assurance | • Automatic Collision Notification and Assistance • SOS Emergency Assist • Enhanced Roadside Assist • Monthly Vehicle Report
Essentials | • Convenience: – Remote Door Lock – Remote Door Unlock – Remote Horn/Lights – Remote Vehicle Start*
– Quick Tips
– Location Sharing
– Voice Text Messaging
• Vehicle Self Diagnostics:
– Automatic Diagnostics Trouble Code Notification
– Maintenance Alert
– Recall Advisor
– Service Link
• Safeguard:
– Stolen Vehicle Recovery
– Stolen Vehicle Slowdown
– Vehicle Immobilization
– Valet Alert
– Panic Notification
– Alarm Notification
– Geo-Fence
– Speed Alert
– Curfew Alert
Guidance | • Point of Interest Search by Advanced Voice Recognition • Point of Interest Web Search & Download • Turn-by-Turn Navigation** • Daily Route Guidance with Traffic Conditions • Traffic
• Gas Station Locations & Gas Prices
• Eco-Coach
• Restaurant Ratings & Locations
• Weather

Owners can subscribe to Blue Link packages in the following groupings;

A. | Assurance

B. | Assurance + Essentials

C. | Assurance + Essentials + Guidance

3. | Setting Blue Link preferences Many Blue Link features, reports, or alerts require setup, with input from you.

For more detail procedure, please refer to the Blue Link owner's manual.

4. | Accessing Blue Link preferences

(1) | Smart Phone Mobile Application You can download the Blue Link mobile app to your compatible smart phone. For more detail procedure, please refer to the Blue Link owner's manual.

(2) | In-car Application Controls for Blue Link in-vehicle voice-response use are located on the rearview mirror.

For more detail procedure, please refer to the Blue Link owner's manual.

(3) | Web Application Many Blue Link features can be customized, activated, or accessed at www.MyHyundai.com. This is your important link to getting the most out of your Blue Link system.

For more detail procedure, please refer to the Blue Link owner's manual.

Service List

1. | Safety and Security

Service Name | Service Trigger
- Auto Crash Notification | When an accident occurred and airbag deployed, ACN notification will be triggered automatically.
- SOS – Emergency Assistance | It will be triggered by manually pressing the SOS button on the inside mirror. It will connect you to emergency assistance helper.
- Alarm/Panic Notification | when the vehicle alarm system is activated, it will be automatically triggered and inform to owner. If the customer push the panic button of key FOB near the vehicle, it will be triggered and notify that driver or vehicle occupant may be in danger
- Enhanced roadside | Push the Interactive Voice Recognition (IVR) button on the inside mirror and ask to operator about the help.
- Speed Alert | Customer can setup notification limit of vehicle speed on the web or by asking operator using IVR call.
- Remote Door Control – Lock | Customer can ask Remote Door Lock service by using the Smart Phone application or on the web(CWP) or asking to operator by IVR call.
- Remote Door Control – Unlock | Customer can ask Remote Door Unlock service by using the Smart Phone application or on the web(CWP) or asking to operator by IVR call.
- Remote Horn and Lights | Customer can ask Horn&Light or Light Only services by using the Smart Phone application or on the web(CWP) or asking to operator by IVR call.
- Stolen Vehicle Recovery | This service can be triggered on request by police only
- Vehicle Immobilization/Slowdown | This service can be triggered on request by police only
- Curfew Alert | The customer can setup notification time interval that vehicle being used on the web or by asking operator using IVR call.
- Vehicle Remote Start | The customer can ask remote start service by using the Smart Phone application or on the web(CWP) or asking to operator by IVR call. (Automatic transmission only)

2. | Voice Recognition Module (VRM)

Service Name | Service Trigger
- Eco Coach | 1 Showing the eco-coach window. The customer can see the average efficiency curve of fuel consumption by selecting eco-coach software button into the Info menu or saying “eco-coach on” using PTT button on the inside mirror. - Selecting eco-coach button
- Saying “Eco-coach on” menu : Press PTT button on the inside mirror, after heard “Please say command” sound, say “Eco- coach on”
2 See the fuel consumption on the web.
Refer to the telematics web service manual for detail information.
- Maintenance Alert Notification | Refer the telematics web service manual for detail information about setup mile triggered diagnostic service
- Automated DTC notification | If the vehicle found any problem on the vehicle itself, this information will be sent for server automatically.
- Recall and campaign advisor | When any recall or campaign notification for his vehicle is sent by the HMC, it will be shown on the screen. The customer can heard notification by using IVR call, after heard the notification, the popup will be removed automatically.
- Web- Based Diagnostics | The customer can check the status of vehicle using telematics web server. Refer to the telematics web service manual for more information.
- Scheduled Diagnostics | There are two kinds of scheduled diagnostic options. Please see telematics web service manual for more information.

3. | Geographic Information System (GIS)

Service Name | Service Trigger
- Traffic Flow Accident Construction Control | The customer can heard construction or accident condition on the driving road flow using IVR call. Please ask operator after IVR call connected.
- Daily Route Guide with Traffic | The customer can heard traffic comparison between several road using IVR call. Please ask Operator after IVR call connected. Before listen this service, the customer should establish the routes on the web. Refer to the telematics web service manual for more information.
- Gas Station Location and Fuel Prices | The customer can heard Gas station location and Fuel prices using IVR call, and this Point of Interests (POI) information can be downloaded on the vehicle. In case of Audio HU (Standard type), customer
- Geo-Fence | The customer can setup valid boundary of vehicle driving. It can be used for Varlet geo-fence or normal geofence. Both can be setup by web or by asking operator using IVR call.
- Operator Navigation | The customer can heard navigation using IVR call. Please ask "Operator" on the IVR call, and ask your heading
- POI by Guided IVR with Operator Backup | POI download can be requested via IVR call.
- POI Download by Operator | POI download can be requested via IVR call.
- POI Download via Web Portal | POI download can be requested using web portal.
- POI Searching by IVR (TMU and Phone) | POI download can be requested via IVR call.
- Friend Finder | For this service, the customer should pre-registration friend information on the web. When your friend ask inform hi’s/she’s location to you, it can will be download by a kinds of POI.

4. | Operator Service & ETC

Service Name | Service Trigger
- IVR Owner’s Manual | The Customer can heard how to using about any kinds of vehicle Manual. Please ask operator on the IVR call.
- Operator Assisted Owner's Manual | The Customer can heard how to using about any kinds of vehicle Manual. Please ask operator on the IVR call.
- Q-feedback | This is one of diagnostic services. When customer heard any unusual noise on the vehicle, customer can ask checking the vehicle using IVR call.

Service Name | Service Trigger
- Voice Text Messaging |
- Provisioning |
- TMU Disable Mode | “blueLink not active. Please call xxx-xxx-xxxx” will be showing when any button pushed after disable the telematics services.
- TMU Swap | The Proper TMU (TeleMatics Unit) should be installed on the vehicle. “Incorrect Telematics Unit Contact Dealer” will be showing if incorrect TMU is installed.