| SONATA(YF) >2013 > G 2.4 GDI > Driveshaft and axle > General Information>Specifications |

Specification

Engine | T/M | Joint type | Max. permissible angle
Outer | Inner | Outer | Inner
Gasoline 2.0 | M/T | BJ#95 | TJ#95 | 43° | 21°
A/T | BJ#95 | TJ#95 | 43° | 21°
Gasoline 2.4 | M/T | BJ#95 | TJ#95 | 43° | 21°
A/T | BJ#95 | TJ#95 | 43° | 21°

Tightening Torque

Item | N.m | kgf.m | Ib.ft
Front | Wheel nut | 88.2 ~ 107.8 | 9.0 ~ 11.0 | 65.0 ~ 79.5
Drive shaft castle nut | 215.7 ~ 254.9 | 22.0 ~ 26.0 | 159.1 ~ 188.0
Strut assembly lower mounting bolt | 137.2 ~ 156.9 | 14.0 ~ 16.0 | 101.2 ~ 115.7
Brake caliper mounting bolt | 78.4 ~ 98.0 | 8.0 ~ 10.0 | 57.8 ~ 72.3
Wheel speed sensor mounting bolt | 6.8 ~ 10.7 | 0.7 ~ 1.1 | 5.0 ~ 7.9
Brake disc mounting bolt | 4.9 ~ 5.8 | 0.5 ~ 0.6 | 3.6 ~ 4.3
Lower ball joint mounting bolt | 98.0 ~ 117.6 | 10.0 ~ 12.0 | 72.3 ~ 86.7
Tie rod end ball joint nut | 34.3 ~ 44.0 | 3.5 ~ 4.5 | 25.3 ~ 32.5
Rear | Wheel nut | 88.2 ~ 107.8 | 9.0 ~ 11.0 | 65.0 ~ 79.5
Shock absorber upper mounting bolt | 137.2 ~ 156.9 | 14.0 ~ 16.0 | 101.2 ~ 115.7
Shock absorber lower mounting nut | 137.2 ~ 156.9 | 14.0 ~ 16.0 | 101.2 ~ 115.7
Brake caliper mounting bolt | 78.4 ~ 98.0 | 8.0 ~ 10.0 | 57.8 ~ 72.3
Wheel speed sensor mounting bolt | 6.8 ~ 10.7 | 0.7 ~ 1.1 | 5.0 ~ 7.9
Brake disc mounting bolt | 4.9 ~ 5.8 | 0.5 ~ 0.6 | 3.6 ~ 4.3
Hub assembly mounting bolt | 78.4 ~ 88.2 | 8.0 ~ 9.0 | 57.8 ~ 65.0
Upper arm ball joint mounting nut | 137.2 ~ 156.9 | 14.0 ~ 16.0 | 101.2 ~ 115.7
Lower arm mounting bolt | 137.2 ~ 156.9 | 14.0 ~ 16.0 | 101.2 ~ 115.7
Assist arm ball joint mounting nut | 44.1 ~ 53.9 | 4.5 ~ 5.5 | 32.5 ~ 39.7
Trailing arm mounting bolt | 44.1 ~ 53.9 | 4.5 ~ 5.5 | 32.5 ~ 39.7

Lubricants

Engine | Lubricants | Quantity
Gasoline 2.0 | BJ | GRB006 (UREA) | 105g
TJ | SH06-VX21(UREA) | 145g
Gasoline 2.4 | BJ | GRB006 (UREA) | 105g
TJ | SH06-VX21(UREA) | 145g