| SONATA(YF) >2012 > G 2.4 GDI > Driveshaft and axle > General Information>Troubleshooting |

Troubleshooting

Trouble Symptom | Probable cause | Remedy
Vehicle pulls to one side | Scoring of driveshaft ball joint | Replace
Wear, rattle or scoring of wheel bearing | Replace
Defective front suspension and steering | Adjustment or Replace
Vibration | Wear, damage or bending of driveshaft | Replace
Driveshaft rattle and hub serration | Replace
Wear, rattle or scratching of wheel bearing | Replace
Shimmy | Defective wheel balance | Adjustment or Replace
Defective front suspension and steering | Adjustment or Replace
Excessive noise | Wear, damage or bending of driveshaft | Replace
Rattle of driveshaft and worn hub splines | Replace
Wear, rattle or scoring of wheel bearing | Replace
Loose hub nut | Adjustment or Replace
Defective front suspension and steering | Adjustment or Replace