| SONATA(YF) >2013 > G 2.4 GDI > Body (Interior and Exterior) > Interior > Roof Trim>Repair procedures |

Replacement

Sunvisor Replacement

• | When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.

• | Put on gloves to protect your hands.

1. | Loosen the mounting screws, then remove the sunvisor (A) and retainer (B).

2. | Installation is the reverse of removal.

Assist Handle Replacement

• | When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.

• | Put on gloves to protect your hands.

1. | Remove the covers (A) and screws, then remove the assist handle (B).

2. | Installation is the reverse of removal.

Overhead Console Lamp Replacement

• | When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.

• | Put on gloves to protect your hands.

1. | After loosening the mounting screws, remove the overhead console (A).

2. | Disconnect the connectors (B).

3. | Installation is the reverse of removal.

Room Lamp Replacement

• | When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.

• | Put on gloves to protect your hands.

1. | Remove the covers (A).

2. | After loosening the mounting screws, then remove the room lamp (B).

3. | Disconnect the connector (A).

4. | Installation is the reverse of removal.

Hends Free Mic and Lamp Replacement

1. | Remove the hands free mic (A) and lamp (B).

2. | Installation is the reverse of removal.

Roof Trim Replacement

• | Put on gloves to protect your hands.

• | When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.

• | Take care not to bend or scratch the trim and panels.

1. | Remove the following items :

A. | Rear seat cushion (Refer to the BD group - "Rear Seat")

B. | Front door scuff trim & Rear door scuff trim (Refer to the BD group - "Interior Trim")

C. | Front pillar trim (Refer to the BD group - "Interior Trim")

D. | Center pillar lower trim & Center pillar upper trim (Refer to the BD group - "Interior Trim")

E. | Rear pillar trim (Refer to the BD group - "Interior Trim")

F. | Sunvisor

G. | Overhead console

H. | Room lamp

I. | Assist handle

2. | Disconnect the connector (A). [Driver's] [Passenger's]

3. | Disconnect the clips.

4. | Remove the roof trim (A).

5. | Installation is the reverse of removal.

• | Replace any damage clips.