| SONATA(YF) >2013 > G 2.4 GDI > Body Electrical System > AVN System > AVN Head Unit>Components and Components Location |

Components

AVN (A/V & Navigation) Head Unit Connector

Pin No. | Connector A | Connector B
Description | Remarks | Description | Remarks
1 | - | - | CAN H | Used for CAN network
2 | - | - | - | -
3 | - | - | - | -
4 | - | - | Steering remote control | Steel wheel remote control input
5 | SP DIF ground | To EXT AMP | - | -
6 | SP DIF (+) | To EXT AMP | - | -
7 | ALT | ALT L | - |
8 | Illumination (+) | Rheostat from vehicle (+) | AUX input (RH) | AUX ST Sound R-CH Input
9 | R Position | R Signal | AUX Ground | AUX ST sound ground
10 | - | - | MIC+ (Bluetooth) | Bluetooth hand free
11 | - | - | ACC (+) | ACC
12 | NAVI AMP (-) | Used for voice recognition | Battery (+) | Fused battery power supply (10A)
13 | NAVI AMP (+) | Used for voice recognition | CAN L | Used for CAN NETWORK
14 | - |  | Auto right | Auto right signal input
15 | SP DIF (-) | To EXT AMP | P Position | P Position(TGS) signal from vehicle
16 | DOOR | Door unlock signal | Speed | Speed signal from vehicle
17 | Illumination (-) | Rheostat from vehicle (-) | Steering remote ground | Steel wheel remote control input
18 | Remote antenna | Remote supply for motorised antenna | - | -
19 |  | - | -
20 | AUX DETECT | AUX connection DETECT
21 | AUX input (LH) | AUX ST SOUND L-CH Input
22 | MIC- (Bluetooth) | Bluetooth hand free
23 | Ground | Ground
24 | Ground | Ground