Attention: this file have to decode, before the used, with algorithm Siemens F200.

These are the operations you have to do:

1. read the original file and save it on hard disk
2. by Tools menu of ECM TITANIUM select ENCODINGS->SIEMENS --> F200 --> Decode > BIN
3. the decode file will be saved with extension .BIN in the same directory of the original file.

NB: If you use the emulator the type of eprom is: MS42F400

At the end of the work is necessary to recodify the modificated file after the saving with ECM TITANIUM as follows:

1. by Tools menu of ECM TITANIUM select ENCODINGS->SIEMENS --> F200 --> Coding > SIE
2. the codify will be saved with extension .SIE in the same of the modificated file.

DURING THE PROGRAMMING OF THE EPROM YOU MUSTN'T PROTECT THE SECTORS

After each modification, it is mandatory to read the EPROM again, then to start working on the last file read