Attention: in this file using family 01 Bosch Edc 29F200 checksum find an error on original file

Do in the following case:

1. Read the original file and save it on disk
2. Go in the Tools menu, settings, and select item overwrite similar maps
3. Execute the map with ECM TITANIUM using the right driver always modifing the similar map 1
4. Save file on disk
5. exit and enterin the program without open driver
6. load original and modify files and put the values at following adresses : EFFC-EFFD-EFFE-EFFF
7. save and program eprom now.