Attention: this file has to be decoded, before to be used, with algorithm Siemens F200 only if you use the eprom programmer.

If you use the Kess to read the eprom, you have to:

1. read the complete file and save it on the hard disk. In this way you will obtain an empty file that contains only the data list. Now the file is ready to be used with ECM TITANIUM.

Instead, if you use the eprom programmer to read the eprom, you have to:

1. read the original file and save it on the hard disk

2. by Tools menu of ECM TITANIUM select ENCODINGS->SIEMENS --> F200 --> Decode > BIN

3. the decoded file will be saved with extension .BIN in the same directory of the original file.

Note: If you use the emulator the type of eprom to be used is: 5WP4F200 or 5WP4F400 according to the size of the eprom.

Instead, if you use the Kess to rewrite the eprom you have to:

1. don't codify the file, it is ready for writing

If you use the eprom programmer, at the end of the work it is necessary to recodify the modified file after saving it with ECM TITANIUM as follows:

1. by Tools menu of ECM TITANIUM select ENCODINGS->SIEMENS --> F200 --> Coding > SIE

2. The codified file will be saved with extension .SIE in the same directory of the modified file.